|  |  |
| --- | --- |
| Product Name: | AFPP-23-TS |
|  |  |
| Description: | VWR Catalog No.10819-492  VWR Performance Auto Defrost Stainless Steel Laboratory Freezer  23 Cu. Ft. Capacity  One swing stainless steel door  Multi-Point temperature mapping via NIST traceable data acquisition, 15 probes in air and 3 probes in sample solution for 360 minutes with temperature readings every 60 seconds  Enhanced operation manual  TempData-2000 Touch Screen Digital Temperature Display & Alarm Module:  Password-protected touchpad membrane control panel  Sample simulated digital temperature display: .1° resolution, adjustable temperature display in Celsius or Fahrenheit  Audible and visual high/low temperature alarms  Sensor error alarm  Power failure alarm  Door ajar alarm  Low battery alarm  Operation indicator  Active temperature scale bar display  Resettable 1-point min/max history  24-hour temperature chart  Temperature & alarm event data logging  USB port for data transfer and software updates  Real-time operational display clock  4-20mA output  Remote alarm contacts  Alarm validation (audible, visual, and remote alarms)  Alarm ring back  Adjustable alarm volume  Troubleshooting guide  Owner’s Manual & Technical Support Contact Information  Adjustable operating temperature range: -15°C – -25°C  Three shelves (adjustable in ½" increments)  Keyed door lock  Magnetic door gasket for positive seal  Recessed door handle  Swivel casters (adds 5" to height)  Interior light  Probe access port (3/8")  300 Series stainless steel interior/exterior  High density urethane foam cabinet and door insulation  HFC-free refrigerant (R290a), foam insulation and packaging  Quality certified with 100% unit temperature testing  Three year parts and labor warranty, plus an additional two year compressor parts warranty  Exterior dimensions: 27” W x 29 ½ “D x 78 5/16"H without casters; 83 5/16”H with casters Auto defrost  115V, 60 Hz, 5.5 Amps,1/2 HP  Shipping weight: 285 lbs. |