|  |  |
| --- | --- |
| Product Name: | AFPP-23-TS |
|  |  |
| Description: | VWR Catalog No.10819-492VWR Performance Auto Defrost Stainless Steel Laboratory Freezer23 Cu. Ft. CapacityOne swing stainless steel doorMulti-Point temperature mapping via NIST traceable data acquisition, 15 probes in air and 3 probes in sample solution for 360 minutes with temperature readings every 60 secondsEnhanced operation manualTempData-2000 Touch Screen Digital Temperature Display & Alarm Module:Password-protected touchpad membrane control panelSample simulated digital temperature display: .1° resolution, adjustable temperature display in Celsius or FahrenheitAudible and visual high/low temperature alarmsSensor error alarmPower failure alarmDoor ajar alarmLow battery alarmOperation indicatorActive temperature scale bar displayResettable 1-point min/max history24-hour temperature chartTemperature & alarm event data loggingUSB port for data transfer and software updatesReal-time operational display clock4-20mA outputRemote alarm contactsAlarm validation (audible, visual, and remote alarms)Alarm ring backAdjustable alarm volumeTroubleshooting guideOwner’s Manual & Technical Support Contact InformationAdjustable operating temperature range: -15°C – -25°C Three shelves (adjustable in ½" increments)Keyed door lockMagnetic door gasket for positive sealRecessed door handleSwivel casters (adds 5" to height)Interior lightProbe access port (3/8")300 Series stainless steel interior/exteriorHigh density urethane foam cabinet and door insulationHFC-free refrigerant (R290a), foam insulation and packagingQuality certified with 100% unit temperature testingThree year parts and labor warranty, plus an additional two year compressor parts warrantyExterior dimensions: 27” W x 29 ½ “D x 78 5/16"H without casters; 83 5/16”H with castersAuto defrost115V, 60 Hz, 5.5 Amps,1/2 HPShipping weight: 285 lbs. |